     .--------. .--------.   .---.
     `-----.   |`------.  `.  \   \
           |   |        |  |.--    \
           |   |.------'  .`----.   \
           `---'`---------'      `---'

<< E L E C T R O L U M I N E S C E N C E >>
.-----------------------------------------.

A real  wild demo for  Assembly Summer 2023
by TDA feat. HwOps.

 Code            Firehawk, Kamihaze, Kriel 
 Hardware        Firehawk, Kamihaze
 Music           Preda

Runs on a large  DIY 16x16 pixel WS2813 LED
screen,  controlled  by a  Raspberry Pi 400
through  a  custom  interface  board.   The
display is built primarily from  MDF board,
3D-printed  parts and  polycarbonate sheet.

Provided  RPi Linux armv7l  binaries  drive
the  WS281x   LED  chain  on  GPIO18.   Run
the executable  with  command line flag  -h
to see the available options for displaying
on an LED screen.  The demo can render both
to an SDL window and an LED screen.

Additional    executable    binaries    are 
included  for  MacOS  (x86-64  and  arm64),
Linux  (x86-64)  and  Windows.  These  only
render  to an  emulated  screen  in an  SDL
window.

All executables have been dynamically linked
against SDL2 libraries, so install them from
apt/pacman/homebrew/etc to run the demo.

Go modules used:
   * rpi-ws281x-go by supcik and jgarff
   * go-sdl2 by veandco and the SDL project
   * minimp3 by tosone and lieff
   * go3d by ungerik
'-----------------------------------------'