```
mystery_disk_lpp_basf-5.25-2s2d-48tpi_720k.img
mystery_disk_lpp_basf-5.25-2s2d-48tpi_720k.scp
mystery_disk_lpp_basf-5.25-2s2d-48tpi_720k_hexdump.txt
	BASF 2S/2D 48tpi disk, read at heads=2, tracks=80, sectors=18,
	256 bytes per sector, MFM encoding. Single bad sector at h=1,t=59.

mystery_eprom_1_tms-27c128.bin
mystery_eprom_2_am27c128.bin
mystery_eprom_3_nm27c64q.bin
mystery_eprom_4_w29ee011.bin
mystery_eprom_5_w27c512.bin
mystery_eprom_6_mbm27128.bin
mystery_eprom_7_mbm27128.bin
	Unknown ROM/EPROM/EEPROM chips from parts bin.

mystery_eprom_8_mx29f040c.bin
	EEPROM from Omega MSX chip kit.
```
